|  |
| --- |
| **Contractor Bid Form for 11-Mile Canyon Diversion Dam Removal Project (70% Design Quantities)** |
| \*During final design, the Bid Items, Measurement, and Payment will be updated to follow Colorado Dept. of Transportation Specifications. |
| \*Contractor may submit documentation for the basis of the bid, assumptions made, or other notes if desired. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **BID ITEM** | **BID ITEM DESCRIPTION** | **QUANTITY** | **PAY UNIT** | **UNIT COST** | **COST** |
| 1 | Mobilization | 1 | LS |  |  |
| 2 | Traffic and Pedestrian Control (Special) | 1 | LS |  |  |
| 3 | Plastic Mesh Construction Fence | 4,300 | LF |  |  |
| 4 | Construction Surveying | 1 | LS |  |  |
| 5 | Vehicle Tracking Pad | 3 | EACH |  |  |
| 6 | Stabilized Staging Area | 6,200 | SY |  |  |
| 7 | Tree/Plant Protection Fence | 900 | LF |  |  |
| 8 | Rock Check Dam | 1 | EACH |  |  |
| 9 | Sediment Control Log | 7,500 | LF |  |  |
| 10 | Silt Fence (Reinforced) | 275 | LF |  |  |
| 11 | Access Road and Turnaround Area Stabilization | 1 | LS |  |  |
| 12 | Clearing and Grubbing (Dam Area and Fill Areas) | 10.5 | ACRE |  |  |
| 13 | Water Control (Coffer Dam, Diversion Channel, Crossings) | 1 | LS |  |  |
| 14 | Removal of Tree and Use for Habitat | 10 | EACH |  |  |
| 15 | Remove/Dispose of Outhouse | 1 | EACH |  |  |
| 16 | Remove/Dispose of Dam, Fishing Pier, and All Appurtenances | 1 | LS |  |  |
| 17 | Remove/Dispose of Trail Riprap | 80 | SY |  |  |
| 18 | Remove/Dispose of Channel Riprap | 160 | SY |  |  |
| 19 | Cap Existing Steel Pipe to be Abandoned | 1 | EACH |  |  |
| 20 | Strip, Stockpile, Amend, and Replace 6-Inch Topsoil | 4,200 | CY |  |  |
| 21 | Excavation and Place On Site | 20,000 | CY |  |  |
| 22 | Riffle / Drop / Pool Features | 5 | EACH |  |  |
| 23 | Import Cobble/Gravel for Substrate | 630 | CY |  |  |
| 24 | Screen On-Site Cobbles/Gravel for Substrate | 950 | CY |  |  |
| 25 | Rootwad/Toe Wood Structure | 4 | EACH |  |  |
| 26 | Boulder Cluster (from on-site) | 20 | TON |  |  |
| 27 | Mulch (Weed Free Straw) | 6 | ACRE |  |  |
| 28 | Seeding (Riparian) | 0.6 | ACRE |  |  |
| 29 | Seeding (Floodplain) | 0.7 | ACRE |  |  |
| 30 | Seeding (Upland Forest) | 4.6 | ACRE |  |  |
| 31 | Erosion Control Blanket | 10,800 | SY |  |  |
| 32 | Wetland Plug - 10-Inch Conetainer | 30,000 | EACH |  |  |
| 33 | Shrubs, 4-Inch by 14-Inch Treepot (Willow Stakes) | 200 | EACH |  |  |
| 34 | Shrubs, 5-Gallon Container | 60 | EACH |  |  |
| 35 | Transplant Existing Wetlands | 100 | SY |  |  |
| 36 | Upland Tree, Evergreen, 6-Foot Height, Ball and Burlap | 12 | EACH |  |  |
| 37 | Fence Combination Wire with Metal Posts | 250 | LF |  |  |
| **TOTAL** |  |

|  |
| --- |
| Company Namet:$  |

|  |
| --- |
| Total Bid Amount: $  |
| (numbers) |

|  |  |
| --- | --- |
| Total Bid Amount:  | **Dollars** |
| (words) |  |  |
| Signature (approved signer):  | Title:  |